telemetry.internal.platform.power_monitor.msr_power_monitor | index telemetry/internal/platform/power_monitor/msr_power_monitor.py

`# Copyright 2014 The Chromium Authors. All rights reserved.
# Use of this source code is governed by a BSD-style license that can be
# found in the LICENSE file.`

Modules
`` |  |
telemetry.decorators logging | platform telemetry.internal.platform.power_monitor | re |

Classes
`` |  | telemetry.internal.platform.power_monitor.PowerMonitor(__builtin__.object) MsrPowerMonitor MsrPowerMonitorLinux MsrPowerMonitorWin
class MsrPowerMonitor(telemetry.internal.platform.power_monitor.PowerMonitor)
`` |  | Method resolution order: MsrPowerMonitor telemetry.internal.platform.power_monitor.PowerMonitor __builtin__.object Methods defined here: CanMonitorPower(self) StartMonitoringPower(self, browser) StopMonitoringPower(self) __init__(self, backend) Methods inherited from telemetry.internal.platform.power_monitor.PowerMonitor: CanMeasurePerApplicationPower(self) `Returns True if the power monitor can measure power for the target application in isolation. False if power measurement is for full system energy consumption.` Data descriptors inherited from telemetry.internal.platform.power_monitor.PowerMonitor: __dict__ `dictionary for instance variables (if defined)` __weakref__ `list of weak references to the object (if defined)`
class MsrPowerMonitorLinux(MsrPowerMonitor)
`` |  | Method resolution order: MsrPowerMonitorLinux MsrPowerMonitor telemetry.internal.platform.power_monitor.PowerMonitor __builtin__.object Methods defined here: CanMonitorPower(self) Methods inherited from MsrPowerMonitor: StartMonitoringPower(self, browser) StopMonitoringPower(self) __init__(self, backend) Methods inherited from telemetry.internal.platform.power_monitor.PowerMonitor: CanMeasurePerApplicationPower(self) `Returns True if the power monitor can measure power for the target application in isolation. False if power measurement is for full system energy consumption.` Data descriptors inherited from telemetry.internal.platform.power_monitor.PowerMonitor: __dict__ `dictionary for instance variables (if defined)` __weakref__ `list of weak references to the object (if defined)`
class MsrPowerMonitorWin(MsrPowerMonitor)
`` |  | Method resolution order: MsrPowerMonitorWin MsrPowerMonitor telemetry.internal.platform.power_monitor.PowerMonitor __builtin__.object Methods defined here: CanMonitorPower(self) StopMonitoringPower(self) Methods inherited from MsrPowerMonitor: StartMonitoringPower(self, browser) __init__(self, backend) Methods inherited from telemetry.internal.platform.power_monitor.PowerMonitor: CanMeasurePerApplicationPower(self) `Returns True if the power monitor can measure power for the target application in isolation. False if power measurement is for full system energy consumption.` Data descriptors inherited from telemetry.internal.platform.power_monitor.PowerMonitor: __dict__ `dictionary for instance variables (if defined)` __weakref__ `list of weak references to the object (if defined)`

Data
`` |  | IA32_PACKAGE_THERM_STATUS = 433 IA32_TEMPERATURE_TARGET = 418 MSR_DRAM_ENERGY_STATUS = 1561 MSR_PKG_ENERGY_STATUS = 1553 MSR_PP0_ENERGY_STATUS = 1593 MSR_PP1_ENERGY_STATUS = 1601 MSR_RAPL_POWER_UNIT = 1542